(footprint "Relay_SPST_Omron_G5NB"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PCB Power Relay, SPST-NO, 7A (250 VAC), 5A (30 VDC), 20.5x7.2x15.3mm max")
	(tags "Omron G5NB Relay SPST-NO")
	(property "Reference" "REF**"
		(at 9.25 -2.64 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_SPST_Omron_G5NB"
		(at 9.25 7.05 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 9.25 2.35 180)
		(layer "F.Fab")
	)
	(pad "13" thru_hole oval
		(at 11.5 4.7 180)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole oval
		(at 18.5 4.7 180)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole rect
		(at 0 0 180)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A2" thru_hole oval
		(at 0 4.7 180)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPST_Omron_G5NB.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
