(footprint "Relay_SPST_Omron_G5PZ"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Relay Omron G5PZ, see https://components.omron.com/us-en/sites/components.omron.com.us/files/datasheet_pdf/K320-E1.pdf")
	(tags "Relay Omron G5PZ")
	(property "Reference" "REF**"
		(at 0.75 -3.1 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_SPST_Omron_G5PZ"
		(at 4 8 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" "https://components.omron.com/us-en/sites/components.omron.com.us/files/datasheet_pdf/K320-E1.pdf"
		(at 3.75 10 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 7.5 0 270)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at -1.3 8.7 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "13" thru_hole circle
		(at 0 16.5 90)
		(size 2.1 2.1)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 7.5 20 90)
		(size 2.1 2.1)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole roundrect
		(at 0 0 90)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.1388888889)
	)
	(pad "A2" thru_hole circle
		(at 7.5 0 90)
		(size 1.8 1.8)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPST_Omron_G5PZ.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
