(footprint "Relay_SPST_Panasonic_ALFG_FormA"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Panasonic Relay SPST, https://www3.panasonic.biz/ac/e_download/control/relay/power/catalog/mech_eng_lfg.pdf")
	(tags "Panasonic Relay SPST")
	(property "Reference" "REF**"
		(at 12.5 -3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_SPST_Panasonic_ALFG_FormA"
		(at 12 7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 11.5 4.875 0)
		(layer "F.Fab")
	)
	(pad "11" thru_hole oval
		(at -1.8 12)
		(size 2.1 3.6)
		(drill oval 1.1 2.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole oval
		(at 25.8 12)
		(size 2.1 3.6)
		(drill oval 1.1 2.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole roundrect
		(at 0 0)
		(size 3.1 1.5)
		(drill oval 2.1 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "A2" thru_hole oval
		(at 22 0)
		(size 3.1 1.5)
		(drill oval 2.1 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPST_Panasonic_ALFG_FormA.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
