(footprint "Relay_SPST_RAYEX-L90AS"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://a3.sofastcdn.com/attachment/7jioKBjnRiiSrjrjknRiwS77gwbf3zmp/L90-SERIES.pdf")
	(tags "Relay RAYEX L90AS SPST NO")
	(property "Reference" "REF**"
		(at 12.1666 -14.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_SPST_RAYEX-L90AS"
		(at 18.0594 15.4 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 12.3952 0 0)
		(layer "F.Fab")
	)
	(pad "13" thru_hole circle
		(at 15.2 -8.9 180)
		(size 3 3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 17.74 8.9 180)
		(size 3 3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole roundrect
		(at 2.54 -5.1 180)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "A2" thru_hole circle
		(at 2.54 5.1 180)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPST_RAYEX-L90AS.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
