(footprint "Relay_SPST_Schrack-RP-II-1-FormA_RM5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Relay SPST Schrack-RP-II/1 RM5mm 8A 250V AC Form A http://image.schrack.com/datenblaetter/h_rp810012-b.pdf")
	(tags "Relay SPST Schrack-RP-II/1 RM5mm 8A 250V AC Relay")
	(property "Reference" "REF**"
		(at 13.97 -3.81 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_SPST_Schrack-RP-II-1-FormA_RM5mm"
		(at 12.192 11.43 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 12.065 3.81 0)
		(layer "F.Fab")
	)
	(pad "11" thru_hole circle
		(at 20.32 0)
		(size 3 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 25.32 7.62)
		(size 3 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A2" thru_hole circle
		(at 0 7.62)
		(size 3 3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPST_Schrack-RP-II-1-FormA_RM5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
