(footprint "Relay_SPST_TE_PCH-1xxx2M"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Miniature PCB Relay, PCH Series, 1 Form A (NO), SPST http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Data+Sheet%7FPCH_series_relay_data_sheet_E%7F1215%7Fpdf%7FEnglish%7FENG_DS_PCH_series_relay_data_sheet_E_1215.pdf")
	(tags "Relay SPST NO")
	(property "Reference" "REF**"
		(at 9.5 -2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_SPST_TE_PCH-1xxx2M"
		(at 9 10 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 8.95 3.8 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.155)
	)
	(pad "2" thru_hole circle
		(at 10.2 7.6)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 17.9 7.6)
		(size 2.5 2.5)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 7.6)
		(size 2.2 2.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPST_TE_PCH-1xxx2M.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
