(footprint "Relay_SPST_TE_PCN-1xxD3MHZ"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1461491%7FG2%7Fpdf%7FEnglish%7FENG_CD_1461491_G2.pdf%7F3-1461491-0")
	(tags "SPST relay slim")
	(property "Reference" "REF**"
		(at 9.28 -2.3 180)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_SPST_TE_PCN-1xxD3MHZ"
		(at 9.24 5.79 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 8.75 1.53 0)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -0.4 1.95 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.778 1.778)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.54 0)
		(size 1.778 1.778)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 10.16 0)
		(size 1.9 1.9)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 17.78 0)
		(size 1.9 1.9)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPST_TE_PCN-1xxD3MHZ.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
