(footprint "Relay_Socket_DPDT_Finder_96.12"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DPDT relay socket, 15A max 10A per contact, 2kV AC Isolation, https://gfinder.findernet.com/public/attachments/56/DE/S56DE.pdf")
	(tags "finder relay socket 96.12 56.32")
	(property "Reference" "REF**"
		(at -4.48 -3.83 180)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_Socket_DPDT_Finder_96.12"
		(at 8.35 20.32 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 12.065 8.4 0)
		(layer "F.Fab")
	)
	(pad "11" thru_hole circle
		(at 6.1 3.3)
		(size 4 4)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 16.7 3.3)
		(size 4 4)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 12 3.3)
		(size 4 4)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 6.1 13.3)
		(size 4 4)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 16.7 13.3)
		(size 4 4)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 12 13.3)
		(size 4 4)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole roundrect
		(at 0 0)
		(size 4 4)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "A2" thru_hole circle
		(at 0 16.6)
		(size 4 4)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_Socket_DPDT_Finder_96.12.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
