(footprint "Relay_Socket_DPDT_Omron_PLE08-0"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "29mm Dia, round mounting socket, 10A, 2kV AC / minute, 1e3Mohm, https://www.omron.com.tw/data_pdf/cat/common_sockets_ds_e_6_1_csm1819.pdf?#page=27")
	(tags "tube type relay")
	(property "Reference" "REF**"
		(at -2.4 -5.9 180)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_Socket_DPDT_Omron_PLE08-0"
		(at 12.795732 3.300166 180)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "34x37mm industrial relay area"
		(at 29.305732 21.810166 180)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "31mm Dia for Panel cutout"
		(at 23.395732 -4.299834 180)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 12.795732 5.300166 180)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Relay Pin"
		(at 16.375732 6.400166 180)
		(unlocked yes)
		(layer "User.2")
	)
	(pad "11" thru_hole circle
		(at 7.495566 -7.495566 112.5)
		(size 4.5 4.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole circle
		(at 7.495566 18.095898 247.5)
		(size 4.5 4.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole circle
		(at 0 10.600332 202.5)
		(size 4.5 4.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole circle
		(at 18.095898 -7.495566 247.5)
		(size 4.5 4.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole circle
		(at 18.095898 18.095898 112.5)
		(size 4.5 4.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole circle
		(at 25.591464 10.600332 157.5)
		(size 4.5 4.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole roundrect
		(at 0 0 157.5)
		(size 4.5 4.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "A2" thru_hole circle
		(at 25.591464 0 202.5)
		(size 4.5 4.5)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_Socket_DPDT_Omron_PLE08-0.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
