(footprint "Relay_StandexMeder_UMS"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Standex-Meder SIL-relais, UMS, see http://cdn-reichelt.de/documents/datenblatt/C300/UMS05_1A80_75L_DB.pdf")
	(tags "Standex Meder SIL reed relais")
	(property "Reference" "REF**"
		(at 2.2 -2.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_StandexMeder_UMS"
		(at 2.2 2.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.2 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.52 0)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 3.04 0)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.56 0)
		(size 1 1)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_StandexMeder_UMS.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
