(footprint "Relay_Tyco_V23072_Sealed"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Tyco Electronics Mini Relay K (Sealed Version), length 16.9mm, width 14.7mm, height 19.2mm, drill hole 1.30mm ( https://www.electrokit.com/upload/product/41019/41019252/V23072.pdf )")
	(tags "SPST SPDT DC TE0598-P2")
	(property "Reference" "REF**"
		(at 5.4996 -4.064 180)
		(layer "F.SilkS")
	)
	(property "Value" "Relay_Tyco_V23072_Sealed"
		(at 5.08 16.002 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 3.62 -1.52 270)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 3.62 -1.52 270)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 5.08 5.842 180)
		(layer "F.Fab")
	)
	(pad "3" thru_hole circle
		(at 0 12.7 90)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 5.08 0 90)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0 8.89 90)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 10.16 12.7 90)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 10.16 8.89 90)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A1" thru_hole rect
		(at 0 0 90)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A2" thru_hole circle
		(at 10.16 0 90)
		(size 2.3 2.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_Tyco_V23072_Sealed.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
