(footprint "R_Shunt_Isabellenhuette_BVR4026"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "4-Wire Shunt, SMD 4026, https://www.isabellenhuette.de/fileadmin/Daten/Praezisionswiderstaende/Datenblaetter/BVR.PDF")
	(tags "kelvin-connection")
	(property "Reference" "REF**"
		(at 0 -4.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "R_Shunt_Isabellenhuette_BVR4026"
		(at 0 4.699 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -4.025 -0.85)
		(size 2.55 5.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -4.025 3.2)
		(size 2.55 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at 4.025 3.2)
		(size 2.55 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at 4.025 -0.85)
		(size 2.55 5.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Isabellenhuette_BVR4026.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
