(footprint "R_Shunt_Ohmite_LVK12"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "4 contact shunt resistor")
	(tags "shunt resistor 4 contacts")
	(property "Reference" "REF**"
		(at 0 -3.2 180)
		(layer "F.SilkS")
	)
	(property "Value" "R_Shunt_Ohmite_LVK12"
		(at 0 3.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.1 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.7 -1.375)
		(size 1.1 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.7 -1.375)
		(size 1.1 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0.7 1.375)
		(size 1.1 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.7 1.375)
		(size 1.1 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Ohmite_LVK12.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
