(footprint "R_Shunt_Ohmite_LVK20"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "4 contacts shunt resistor, https://www.ohmite.com/assets/docs/res_lvk.pdf")
	(tags "4 contacts resistor smd")
	(property "Reference" "REF**"
		(at 0.025 -4.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "R_Shunt_Ohmite_LVK20"
		(at 0.05 4.325 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.025 -1.975)
		(size 1.55 2.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 1.025 -1.975)
		(size 1.55 2.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 1.025 1.975)
		(size 1.55 2.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.025 1.975)
		(size 1.55 2.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Shunt_Ohmite_LVK20.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
