(footprint "R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=15.24mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
	(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 15.24mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
	(property "Reference" "REF**"
		(at 7.62 -2.37 0)
		(layer "F.SilkS")
	)
	(property "Value" "R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal"
		(at 7.62 2.37 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.62 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 15.24 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
