(footprint "R_Axial_Shunt_L22.2mm_W9.5mm_PS14.30mm_P25.40mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Resistor, Axial_Shunt series, Box, pin pitch=25.4mm, 5W, length*width*height=22.2*9.5*9.5mm^3, shunt pin pitch = 14.30mm, http://www.vishay.com/docs/30217/cpsl.pdf")
	(tags "Resistor Axial_Shunt series Box pin pitch 25.4mm 5W length 22.2mm width 9.5mm height 9.5mm shunt pin pitch 14.30mm")
	(property "Reference" "REF**"
		(at 12.7 -5.87 0)
		(layer "F.SilkS")
	)
	(property "Value" "R_Axial_Shunt_L22.2mm_W9.5mm_PS14.30mm_P25.40mm"
		(at 12.7 5.87 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 12.7 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 5.55 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 19.85 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 25.4 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Shunt_L22.2mm_W9.5mm_PS14.30mm_P25.40mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
