(footprint "R_Axial_Shunt_L47.6mm_W12.7mm_PS34.93mm_P50.80mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Resistor, Axial_Shunt series, Box, pin pitch=50.8mm, 15W, length*width*height=47.6*12.7*12.7mm^3, shunt pin pitch = 34.93mm, http://www.vishay.com/docs/30217/cpsl.pdf")
	(tags "Resistor Axial_Shunt series Box pin pitch 50.8mm 15W length 47.6mm width 12.7mm height 12.7mm shunt pin pitch 34.93mm")
	(property "Reference" "REF**"
		(at 25.4 -7.47 0)
		(layer "F.SilkS")
	)
	(property "Value" "R_Axial_Shunt_L47.6mm_W12.7mm_PS34.93mm_P50.80mm"
		(at 25.4 7.47 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 25.4 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 7.935 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 42.865 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 50.8 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Shunt_L47.6mm_W12.7mm_PS34.93mm_P50.80mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
