(footprint "R_Bare_Metal_Element_L16.3mm_W4.8mm_P15.30mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Resistor, Bare_Metal_Element series, Bare Metal Strip/Wire, Horizontal, pin pitch=15.3mm, 3W, length*width=16.3*4.8mm^2, https://www.bourns.com/pdfs/PWR4412-2S.pdf")
	(tags "Resistor Bare_Metal_Element series Bare Metal Strip Wire Horizontal pin pitch 15.3mm 3W length 16.3mm width 4.8mm ")
	(property "Reference" "REF**"
		(at 7.65 -3.52 0)
		(layer "F.SilkS")
	)
	(property "Value" "R_Bare_Metal_Element_L16.3mm_W4.8mm_P15.30mm"
		(at 7.65 3.52 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.65 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 15.3 0)
		(size 3 3)
		(drill 1.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Bare_Metal_Element_L16.3mm_W4.8mm_P15.30mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
