(footprint "R_Box_L26.0mm_W5.0mm_P20.00mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Resistor, Box series, Radial, pin pitch=20.00mm, 10W, length*width=26.0*5.0mm^2, http://www.produktinfo.conrad.com/datenblaetter/425000-449999/443860-da-01-de-METALLBAND_WIDERSTAND_0_1_OHM_5W_5Pr.pdf")
	(tags "Resistor Box series Radial pin pitch 20.00mm 10W length 26.0mm width 5.0mm")
	(property "Reference" "REF**"
		(at 10 -3.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "R_Box_L26.0mm_W5.0mm_P20.00mm"
		(at 10 3.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 10 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.8 2.8)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 20 0)
		(size 2.8 2.8)
		(drill 1.4)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Box_L26.0mm_W5.0mm_P20.00mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
