(footprint "R_Box_L8.4mm_W2.5mm_P5.08mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Resistor, Box series, Radial, pin pitch=5.08mm, 0.5W = 1/2W, length*width=8.38*2.54mm^2, http://www.vishay.com/docs/60051/cns020.pdf")
	(tags "Resistor Box series Radial pin pitch 5.08mm 0.5W = 1/2W length 8.38mm width 2.54mm")
	(property "Reference" "REF**"
		(at 2.54 -2.52 0)
		(layer "F.SilkS")
	)
	(property "Value" "R_Box_L8.4mm_W2.5mm_P5.08mm"
		(at 2.54 2.52 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.54 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 5.08 0)
		(size 1.6 1.6)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Box_L8.4mm_W2.5mm_P5.08mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
