(footprint "R_Radial_Power_L12.0mm_W8.0mm_P5.00mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Resistor, Radial_Power series, Radial, pin pitch=5.00mm, 3W, length*width=12.0*8.0mm^2, http://www.vishay.com/docs/30218/cpcx.pdf")
	(tags "Resistor Radial_Power series Radial pin pitch 5.00mm 3W length 12.0mm width 8.0mm")
	(property "Reference" "REF**"
		(at 2.5 -5.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "R_Radial_Power_L12.0mm_W8.0mm_P5.00mm"
		(at 2.5 5.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 2.5 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 2.4 2.4)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 5 0)
		(size 2.4 2.4)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Radial_Power_L12.0mm_W8.0mm_P5.00mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
