(footprint "RotaryEncoder_Alps_EC12E_Vertical_H20mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Alps rotary encoder, EC12E..., vertical shaft, http://www.alps.com/prod/info/E/HTML/Encoder/Incremental/EC12E/EC12E1240405.html")
	(tags "rotary encoder")
	(property "Reference" "REF**"
		(at 2.8 -4.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "RotaryEncoder_Alps_EC12E_Vertical_H20mm"
		(at 7.5 10.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 11.5 6.6 0)
		(layer "F.Fab")
	)
	(pad "A" thru_hole rect
		(at 0 0)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B" thru_hole circle
		(at 0 5)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C" thru_hole circle
		(at 0 2.5)
		(size 2 2)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole rect
		(at 7.5 -3.1)
		(size 3 2.5)
		(drill oval 2.5 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole rect
		(at 7.5 8.1)
		(size 3 2.5)
		(drill oval 2.5 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Rotary_Encoder.3dshapes/RotaryEncoder_Alps_EC12E_Vertical_H20mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
