(footprint "RotaryEncoder_Bourns_Vertical_PEC12R-3x17F-Nxxxx"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Bourns rotary encoder, PEC12R, without switch, with bushing, vertical shaft, 17.5mm shaft, https://www.bourns.com/docs/product-datasheets/pec12r.pdf")
	(tags "rotary encoder")
	(property "Reference" "REF**"
		(at 3 -4.75 180)
		(layer "F.SilkS")
	)
	(property "Value" "RotaryEncoder_Bourns_Vertical_PEC12R-3x17F-Nxxxx"
		(at 7.5 11 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7.6 2.5 180)
		(layer "F.Fab")
	)
	(pad "A" thru_hole roundrect
		(at 0 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.15625)
	)
	(pad "B" thru_hole circle
		(at 0 5)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C" thru_hole circle
		(at 0 2.5)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 7.5 -3.1)
		(size 4.1 3)
		(drill oval 3.1 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 7.5 8.1)
		(size 4.1 3)
		(drill oval 3.1 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Rotary_Encoder.3dshapes/RotaryEncoder_Bourns_Vertical_PEC12R-3x17F-Nxxxx.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
