(footprint "RotaryEncoder_Bourns_Vertical_PEL12D-4xxxF-Sxxxx"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Rotary encoder with switch and illuminated 4,6,8,13,18mm shaft, dual-led, https://www.bourns.com/docs/product-datasheets/PEL12D.pdf")
	(tags "rotary encoder illuminated switch vertical")
	(property "Reference" "REF**"
		(at 2.2 -4.4 180)
		(layer "F.SilkS")
	)
	(property "Value" "RotaryEncoder_Bourns_Vertical_PEL12D-4xxxF-Sxxxx"
		(at 0 12.7 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 90)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 90)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 7 3 180)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0 90)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 0 2 90)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 4 90)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 6 90)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "A" thru_hole circle
		(at 14.5 5.5 90)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "B" thru_hole circle
		(at 14.5 3 90)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "C" thru_hole circle
		(at 14.5 0.5 90)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 7 -2.6 90)
		(size 2.8 3.4)
		(drill oval 2 2.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 7 8.6 180)
		(size 3.4 2.8)
		(drill oval 2.6 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Rotary_Encoder.3dshapes/RotaryEncoder_Bourns_Vertical_PEL12D-4xxxF-Sxxxx.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
