(footprint "SPEC_110-xxx_SMD-10Pin_20x20mm_P4.0mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SPEC Sensors SMD package, 20x20mm, https://www.spec-sensors.com/wp-content/uploads/2016/10/3SP_H2S_50-C-Package-110-304.pdf")
	(tags "SPEC Sensors gas sensor")
	(property "Reference" "REF**"
		(at 0 -12 0)
		(layer "F.SilkS")
	)
	(property "Value" "SPEC_110-xxx_SMD-10Pin_20x20mm_P4.0mm"
		(at 0 12 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_line
		(start -7.875 -2.415)
		(end -7.875 2.415)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 2.415 -7.875)
		(end -2.415 -7.875)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 2.415 7.875)
		(end -2.415 7.875)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 7.875 -2.415)
		(end 7.875 2.415)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -7.875 -2.415)
		(mid -7.341934 -3.701934)
		(end -6.055 -4.235)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -6.055 4.235)
		(mid -7.341934 3.701934)
		(end -7.875 2.415)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -6.055 4.235)
		(mid -4.768066 4.768066)
		(end -4.235 6.055)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -4.235 -6.055)
		(mid -4.768066 -4.768066)
		(end -6.055 -4.235)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -4.235 -6.055)
		(mid -3.701934 -7.341934)
		(end -2.415 -7.875)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -2.415 7.875)
		(mid -3.701934 7.341934)
		(end -4.235 6.055)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 2.415 -7.875)
		(mid 3.701934 -7.341934)
		(end 4.235 -6.055)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 4.235 6.055)
		(mid 3.701934 7.341934)
		(end 2.415 7.875)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 4.235 6.055)
		(mid 4.768066 4.768066)
		(end 6.055 4.235)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 6.055 -4.235)
		(mid 4.768066 -4.768066)
		(end 4.235 -6.055)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 6.055 -4.235)
		(mid 7.341934 -3.701934)
		(end 7.875 -2.415)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 7.875 2.415)
		(mid 7.341934 3.701934)
		(end 6.055 4.235)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -8 -9.75)
		(size 1.5 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "2" smd roundrect
		(at -4 -9.75)
		(size 1.5 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "3" smd roundrect
		(at 0 -9.75)
		(size 1.5 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "4" smd roundrect
		(at 4 -9.75)
		(size 1.5 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "5" smd roundrect
		(at 8 -9.75)
		(size 1.5 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "6" smd roundrect
		(at 8 9.75)
		(size 1.5 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "7" smd roundrect
		(at 4 9.75)
		(size 1.5 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "8" smd roundrect
		(at 0 9.75)
		(size 1.5 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "9" smd roundrect
		(at -4 9.75)
		(size 1.5 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(pad "10" smd roundrect
		(at -8 9.75)
		(size 1.5 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1666666667)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Adhes" "F.Paste")
		(name "Keep out")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -6.62 -7.5) (xy -5.38 -7.5) (xy -4.5 -6.62) (xy -4.5 -5.38) (xy -5.38 -4.5) (xy -6.62 -4.5)
				(xy -7.5 -5.38) (xy -7.5 -6.62)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Adhes" "F.Paste")
		(name "Keep out")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -6.62 4.5) (xy -5.38 4.5) (xy -4.5 5.38) (xy -4.5 6.62) (xy -5.38 7.5) (xy -6.62 7.5) (xy -7.5 6.62)
				(xy -7.5 5.38)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Adhes" "F.Paste")
		(name "Keep out")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 5.38 -7.5) (xy 6.62 -7.5) (xy 7.5 -6.62) (xy 7.5 -5.38) (xy 6.62 -4.5) (xy 5.38 -4.5) (xy 4.5 -5.38)
				(xy 4.5 -6.62)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "F.Adhes" "F.Paste")
		(name "Keep out")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 5.38 4.5) (xy 6.62 4.5) (xy 7.5 5.38) (xy 7.5 6.62) (xy 6.62 7.5) (xy 5.38 7.5) (xy 4.5 6.62)
				(xy 4.5 5.38)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor.3dshapes/SPEC_110-xxx_SMD-10Pin_20x20mm_P4.0mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
