(footprint "Sensirion_SCD4x-1EP_10.1x10.1mm_P1.25mm_EP4.8x4.8mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Sensirion SCD4x QFN, 20 Pin (https://sensirion.com/media/documents/C4B87CE6/627C2DCD/CD_DS_SCD40_SCD41_Datasheet_D1.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "Sensirion QFN NoLead")
	(property "Reference" "REF**"
		(at 0 -6.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "Sensirion_SCD4x-1EP_10.1x10.1mm_P1.25mm_EP4.8x4.8mm"
		(at 0 6.05 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -1.2 -1.2)
		(size 1.93 1.93)
		(layers "F.Paste")
		(roundrect_rratio 0.129534)
	)
	(pad "" smd roundrect
		(at -1.2 1.2)
		(size 1.93 1.93)
		(layers "F.Paste")
		(roundrect_rratio 0.129534)
	)
	(pad "" smd roundrect
		(at 1.2 -1.2)
		(size 1.93 1.93)
		(layers "F.Paste")
		(roundrect_rratio 0.129534)
	)
	(pad "" smd roundrect
		(at 1.2 1.2)
		(size 1.93 1.93)
		(layers "F.Paste")
		(roundrect_rratio 0.129534)
	)
	(pad "1" smd roundrect
		(at -4.15 -2.5)
		(size 1.9 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -4.15 -1.25)
		(size 1.9 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -4.15 0)
		(size 1.9 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -4.15 1.25)
		(size 1.9 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -4.15 2.5)
		(size 1.9 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -2.5 4.15)
		(size 0.85 1.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -1.25 4.15)
		(size 0.85 1.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 0 4.15)
		(size 0.85 1.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 1.25 4.15)
		(size 0.85 1.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 2.5 4.15)
		(size 0.85 1.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 4.15 2.5)
		(size 1.9 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 4.15 1.25)
		(size 1.9 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 4.15 0)
		(size 1.9 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 4.15 -1.25)
		(size 1.9 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 4.15 -2.5)
		(size 1.9 0.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 2.5 -4.15)
		(size 0.85 1.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 1.25 -4.15)
		(size 0.85 1.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 0 -4.15)
		(size 0.85 1.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -1.25 -4.15)
		(size 0.85 1.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at -2.5 -4.15)
		(size 0.85 1.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd rect
		(at 0 0)
		(size 4.8 4.8)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(model "${KICAD9_3DMODEL_DIR}/Sensor.3dshapes/Sensirion_SCD4x-1EP_10.1x10.1mm_P1.25mm_EP4.8x4.8mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
