(footprint "Sensortech_MiCS_5x7mm_P1.25mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.sgxsensortech.com/content/uploads/2014/07/1084_Datasheet-MiCS-5524-rev-8.pdf")
	(tags "Sensortech MiCS MEMS sensor")
	(property "Reference" "REF**"
		(at 0 -4.75 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Sensortech_MiCS_5x7mm_P1.25mm"
		(at 0 4.8 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "A" smd rect
		(at -2.25 -1.25 90)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B" smd rect
		(at -2.25 0 90)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C" smd rect
		(at -2.25 1.25 90)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D" smd rect
		(at -1.27 3.25 180)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E" smd rect
		(at 1.25 3.25 180)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F" smd rect
		(at 2.25 1.25 270)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G" smd rect
		(at 2.25 0 270)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H" smd rect
		(at 2.25 -1.25 270)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J" smd rect
		(at 1.27 -3.25 180)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K" smd rect
		(at -1.27 -3.25 180)
		(size 0.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor.3dshapes/Sensortech_MiCS_5x7mm_P1.25mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
