(footprint "Infineon_PG-LLGA-5-2"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Infineon, IP57, XENSIV, LGA-5, https://www.infineon.com/dgdl/Infineon-IM73A135-DataSheet-v01_00-EN.pdf?fileId=8ac78c8c7f2a768a017fadec36b84500")
	(tags "MEMS Microphone LGA Dust Water")
	(property "Reference" "REF**"
		(at 0 -2.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PG-LLGA-5-2"
		(at 0 3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0.03028 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0.68 0 90)
		(size 0.8 0.8)
		(drill 0.8)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" smd roundrect
		(at -1.5 -0.85 270)
		(size 0.75 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.8 -0.85 270)
		(size 0.75 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.5 0.85 270)
		(size 0.75 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -0.8 0.85 270)
		(size 0.75 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd custom
		(at -0.13 0 270)
		(size 0.46 0.46)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_circle
				(center 0 -0.81)
				(end 0.81 -0.81)
				(width 0.46)
				(fill no)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Audio.3dshapes/Infineon_PG-LLGA-5-2.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
