(footprint "InvenSense_ICS-43434-6_3.5x2.65mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TDK InvenSense MEMS I2S Microphone: https://invensense.tdk.com/products/ics-43434/")
	(tags "microphone MEMS I2S ICS-43434 TDK InvenSense")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "InvenSense_ICS-43434-6_3.5x2.65mm"
		(at 0 2.9 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0.01 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 0.71)
		(size 0.5 0.5)
		(drill 0.5)
		(layers "*.Mask")
	)
	(pad "1" smd rect
		(at -0.9 -1.364)
		(size 0.6 0.522)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at -0.9 -0.542)
		(size 0.6 0.522)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd custom
		(at 0.6625 0.71 90)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_circle
				(center 0 -0.6625)
				(end 0.6625 -0.6625)
				(width 0.3)
				(fill no)
			)
		)
	)
	(pad "4" smd rect
		(at 0.9 -0.542)
		(size 0.6 0.522)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" smd rect
		(at 0.9 -1.364)
		(size 0.6 0.522)
		(layers "F.Cu" "F.Mask")
	)
	(pad "6" smd rect
		(at 0 -1.364)
		(size 0.6 0.522)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Audio.3dshapes/InvenSense_ICS-43434-6_3.5x2.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
