(footprint "Knowles_LGA-6_4.72x3.76mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Knowles MEMS Analog Microphone, Omnidirectional, SMD, Differential/Single-Ended Output, -40dB, Bottom Port, https://www.knowles.com/docs/default-source/default-document-library/spm0687lr5h-1_winfrey_datasheet.pdf")
	(tags "SPM0687LR5H MEMS Microphone LGA")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Knowles_LGA-6_4.72x3.76mm"
		(at -0.1 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 0 0.938)
		(size 0.7 0.7)
		(drill 0.7)
		(layers "F&B.Cu" "*.Mask")
	)
	(pad "1" smd circle
		(at -1.204 -1.678)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd circle
		(at -1.265 1.728)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd custom
		(at 0 1.61325)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_circle
				(center 0 -0.67525)
				(end 0.67525 -0.67525)
				(width 0.3255)
				(fill no)
			)
		)
	)
	(pad "4" smd circle
		(at 1.265 1.728)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd circle
		(at 1.204 -1.678)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd circle
		(at 0 -1.678)
		(size 0.9 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Audio.3dshapes/Knowles_LGA-6_4.72x3.76mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
