(footprint "ST_HLGA-6_3.76x4.72mm_P1.65mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.st.com/content/ccc/resource/technical/document/datasheet/group3/27/62/48/98/44/54/4d/36/DM00303211/files/DM00303211.pdf/jcr:content/translations/en.DM00303211.pdf")
	(tags "HLGA Sensor Audio")
	(property "Reference" "REF**"
		(at 0 -3.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "ST_HLGA-6_3.76x4.72mm_P1.65mm"
		(at 0 3.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd circle
		(at -1.17 -1.65)
		(size 0.91 0.91)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd circle
		(at -1.17 0)
		(size 0.91 0.91)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd circle
		(at -1.17 1.65)
		(size 0.91 0.91)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd circle
		(at 1.17 1.65)
		(size 0.91 0.91)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd circle
		(at 1.17 0)
		(size 0.91 0.91)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at 1.17 -1.65 45)
		(size 1.192843 0.91)
		(drill
			(offset -0.141421 0)
		)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Audio.3dshapes/ST_HLGA-6_3.76x4.72mm_P1.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
