(footprint "AKM_CQ_7S"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "AKM Current Sensor, 7 pin, SMD (http://www.akm.com/akm/en/file/datasheet/CQ-236B.pdf)")
	(tags "akm current sensor smd")
	(property "Reference" "REF**"
		(at 0 -5.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "AKM_CQ_7S"
		(at 5 0.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 5 -0.75 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.35 -2.54)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -6.35 -1.27)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -6.35 0)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -6.35 1.27)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -6.35 2.54)
		(size 1.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" thru_hole circle
		(at 3.25 7.43)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 3.95 7.43)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 4.65 7.43)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" smd rect
		(at 5 6.425)
		(size 4.4 2.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" thru_hole circle
		(at 5.35 7.43)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 6.05 7.43)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at 6.75 7.43)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 3.25 -7.43)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 3.95 -7.43)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 4.65 -7.43)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" smd rect
		(at 5 -6.425)
		(size 4.4 2.825)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" thru_hole circle
		(at 5.35 -7.43)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 6.05 -7.43)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at 6.75 -7.43)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Current.3dshapes/AKM_CQ_7S.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
