(footprint "AKM_CZ_SSOP-10_6.5x8.1mm_P0.95mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "AKM CZ-381x current sensor, 6.5x8.1mm body, 0.95mm pitch (http://www.akm.com/akm/en/product/detail/0009/)")
	(tags "akm cz-381x 10")
	(property "Reference" "REF**"
		(at 0 -5 0)
		(layer "F.SilkS")
	)
	(property "Value" "AKM_CZ_SSOP-10_6.5x8.1mm_P0.95mm"
		(at 0 5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -5.29 -3.325)
		(size 1.42 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -5.29 -2.375)
		(size 1.42 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -5.29 -1.425)
		(size 1.42 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -5.29 -0.475)
		(size 1.42 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -5.29 0.475)
		(size 1.42 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -5.29 1.425)
		(size 1.42 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -5.29 2.375)
		(size 1.42 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -5.29 3.325)
		(size 1.42 0.54)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 5.29 1.98)
		(size 1.42 3.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 5.29 -1.98)
		(size 1.42 3.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Current.3dshapes/AKM_CZ_SSOP-10_6.5x8.1mm_P0.95mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
