(footprint "Allegro_CB_PFF"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Allegro MicroSystems, CB-PFF Package (http://www.allegromicro.com/en/Products/Current-Sensor-ICs/Fifty-To-Two-Hundred-Amp-Integrated-Conductor-Sensor-ICs/ACS758.aspx) !PADS 4-5 DO NOT MATCH DATASHEET!")
	(tags "Allegro CB-PFF")
	(property "Reference" "REF**"
		(at 1.91 -16.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Allegro_CB_PFF"
		(at 2.91 -9.7 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0.91 -10.7 90)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.91 0)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 3.82 0)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 2.96 -22.03 65)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 2.96 -20.77 295)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.71 -23.06)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.71 -19.74)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.91 -23.45)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.91 -19.35)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 6.24 -23.45)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 6.24 -19.35)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 6.91 -21.4)
		(size 9 6)
		(drill oval 6 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 7.58 -23.45)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 7.58 -19.35)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 8.91 -23.45)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 8.91 -19.35)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 10.11 -23.06)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 10.11 -19.74)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 10.86 -22.03)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 10.86 -20.77)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -7.04 -22.03)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -7.04 -20.77)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -6.29 -23.06)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -6.29 -19.74)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -5.09 -23.45)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -5.09 -19.35)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -3.76 -23.45)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -3.76 -19.35)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at -3.09 -21.4)
		(size 9 6)
		(drill oval 6 2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -2.42 -23.45)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -2.42 -19.35)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -1.09 -23.45)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -1.09 -19.35)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0.11 -23.06)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at 0.11 -19.74)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 0.86 -22.03 295)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 0.86 -20.77 65)
		(size 0.8 0.8)
		(drill 0.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Current.3dshapes/Allegro_CB_PFF.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
