(footprint "Allegro_CB_PSF"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Allegro MicroSystems, CB-PSF Package (http://www.allegromicro.com/en/Products/Current-Sensor-ICs/Fifty-To-Two-Hundred-Amp-Integrated-Conductor-Sensor-ICs/ACS758.aspx)")
	(tags "Allegro CB-PSF")
	(property "Reference" "REF**"
		(at 1.91 -17.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Allegro_CB_PSF"
		(at 2.91 -9.7 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_line
		(start -3.59 -16.4)
		(end 7.41 -16.4)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -3.59 -2.4)
		(end -3.59 -16.4)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 7.41 -16.4)
		(end 7.41 -2.4)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 7.41 -2.4)
		(end -3.59 -2.4)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at 0.91 -10.7 90)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 1.91 0)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 3.82 0)
		(size 1.5 1.5)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" smd rect
		(at 6.91 -24.6)
		(size 5.5 12)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.09 -24.6)
		(size 5.5 12)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Current.3dshapes/Allegro_CB_PSF.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
