(footprint "Allegro_CB_PSS"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Allegro MicroSystems, CB-PSS Package (http://www.allegromicro.com/en/Products/Current-Sensor-ICs/Fifty-To-Two-Hundred-Amp-Integrated-Conductor-Sensor-ICs/ACS758.aspx)")
	(tags "Allegro CB-PSS")
	(property "Reference" "REF**"
		(at 0 -6.13125 0)
		(layer "F.SilkS")
	)
	(property "Value" "Allegro_CB_PSS"
		(at 1 1.25625 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_line
		(start -5.5 -5.30625)
		(end 5.5 -5.30625)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -5.5 8.69375)
		(end -5.5 -5.30625)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 5.5 -5.30625)
		(end 5.5 8.69375)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 5.5 8.69375)
		(end -5.5 8.69375)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at -1 -0.74375 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.91 15.00625)
		(size 1 9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0 15.00625)
		(size 1 9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 1.91 15.00625)
		(size 1 9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 5 -13.50625)
		(size 5.5 12)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -5 -13.50625)
		(size 5.5 12)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Current.3dshapes/Allegro_CB_PSS.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
