(footprint "Allegro_QSOP-24_3.9x8.7mm_P0.635mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Allegro Microsystems 24-Lead Plastic Shrink Small Outline Narrow Body Body [QSOP] (http://www.allegromicro.com/~/media/Files/Datasheets/ACS726-Datasheet.ashx?la=en)")
	(tags "Allegro QSOP 0.635")
	(property "Reference" "REF**"
		(at 0 -5.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "Allegro_QSOP-24_3.9x8.7mm_P0.635mm"
		(at 0 5.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.5 -3.4925)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.5 -2.8575)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.5 -2.2225)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.5 -1.5875)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.5 -0.9525)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.5 -0.3175)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -2.5 0.3175)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -2.5 0.9525)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -2.5 1.5875)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -2.5 2.2225)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -2.5 2.8575)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -2.5 3.4925)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 2.5 3.4925)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 2.5 2.8575)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 2.5 2.2225)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 2.5 1.5875)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 2.5 0.9525)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 2.5 0.3175)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 2.5 -0.3175)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 2.5 -0.9525)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 2.5 -1.5875)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 2.5 -2.2225)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 2.5 -2.8575)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 2.5 -3.4925)
		(size 2.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/QSOP-24_3.9x8.7mm_P0.635mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
