(footprint "LEM_HO8-NSM"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LEM HO 8/15/25-NSM Current Transducer (https://www.lem.com/sites/default/files/products_datasheets/ho-nsm-0000_series.pdf)")
	(tags "current transducer")
	(property "Reference" "REF**"
		(at 0 -14 0)
		(layer "F.SilkS")
	)
	(property "Value" "LEM_HO8-NSM"
		(at -1 0 90)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(clearance 0.2)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 1.2 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.81 -10.545)
		(size 0.8 4.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.54 -10.545)
		(size 0.8 4.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.27 -10.545)
		(size 0.8 4.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 0 -10.545)
		(size 0.8 4.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.27 -10.545)
		(size 0.8 4.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 2.54 -10.545)
		(size 0.8 4.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 3.81 -10.545)
		(size 0.8 4.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 4.9 1.485)
		(size 5.8 2.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 4.9 4.585)
		(size 5.8 2.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 4.9 7.685)
		(size 5.8 2.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -4.9 7.685)
		(size 5.8 2.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -4.9 4.585)
		(size 5.8 2.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -4.9 1.485)
		(size 5.8 2.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Current.3dshapes/LEM_HO8-NSM.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
