(footprint "LEM_HTFS"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LEM HTFS x00-P current transducer (https://www.lem.com/sites/default/files/products_datasheets/htfs_200_800-p.pdf)")
	(tags "HTFS current transducer")
	(property "Reference" "REF**"
		(at -1.5 -3.5 180)
		(layer "F.SilkS")
	)
	(property "Value" "LEM_HTFS"
		(at 0 9.5 180)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 0 11.5 180)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -16.5 7.12)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -16.5 40.12)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 23.62)
		(size 22 22)
		(drill 22)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 16.5 7.12)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 16.5 40.12)
		(size 1.2 1.2)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.5 1.5)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 0 2.54)
		(size 1.5 1.5)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 0 5.08)
		(size 1.5 1.5)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0 7.62)
		(size 1.5 1.5)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Current.3dshapes/LEM_HTFS.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
