(footprint "Sensirion_DFN-8-1EP_2.5x2.5mm_P0.5mm_EP1.1x1.7mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Sensirion DFN-8 SHT3x-DIS (https://www.sensirion.com/fileadmin/user_upload/customers/sensirion/Dokumente/2_Humidity_Sensors/Datasheets/Sensirion_Humidity_Sensors_SHT3x_Datasheet_digital.pdf)")
	(tags "sensirion dfn nolead")
	(property "Reference" "REF**"
		(at 0 -2.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "Sensirion_DFN-8-1EP_2.5x2.5mm_P0.5mm_EP1.1x1.7mm"
		(at 0 2.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at 0 0)
		(size 0.9 0.9)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.45 0.8) (xy -0.45 0.8) (xy -0.45 -0.53) (xy -0.18 -0.8) (xy 0.45 -0.8)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "1" smd rect
		(at -1.175 -0.75)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.175 -0.25)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.175 0.25)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.175 0.75 180)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.175 0.75)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.175 0.25)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.175 -0.25)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.175 -0.75)
		(size 0.55 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd custom
		(at 0 0)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.5 0.85) (xy -0.5 0.85) (xy -0.5 -0.55) (xy -0.2 -0.85) (xy 0.5 -0.85)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Humidity.3dshapes/Sensirion_DFN-8-1EP_2.5x2.5mm_P0.5mm_EP1.1x1.7mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
