(footprint "CFSensor_XGZP6859D_7x7mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "CFSensor XGZP6859D SO, 6 Pin (https://cfsensor.com/wp-content/uploads/2022/11/XGZP6859D-Pressure-Sensor-V2.5.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "CFSensor SO Sensor_Pressure")
	(property "Reference" "REF**"
		(at 0 -4.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "CFSensor_XGZP6859D_7x7mm"
		(at 0 4.45 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -4.3875 -2.54)
		(size 2.725 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -4.3875 0)
		(size 2.725 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -4.3875 2.54)
		(size 2.725 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 4.3875 2.54)
		(size 2.725 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 4.3875 0)
		(size 2.725 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 4.3875 -2.54)
		(size 2.725 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Pressure.3dshapes/CFSensor_XGZP6859D_7x7mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
