(footprint "CFSensor_XGZP6897x"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Port External Dia 3.13mm, Port Internal Dia 0.9mm, 8 Pin (https://cfsensor.com/wp-content/uploads/2022/11/XGZP6897D-Pressure-Sensor-V2.7.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py, hand modified")
	(tags "sop sensor")
	(property "Reference" "REF**"
		(at 0 -6.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "CFSensor_XGZP6897x"
		(at 0 6.45 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "LP"
		(at -0.9 3.72 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2"
		(at -0.9 2.52 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "HP"
		(at 0.665 -2.47 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "1"
		(at 0.665 -3.67 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -4.6 -3.81)
		(size 2.3 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -4.6 -1.27)
		(size 2.3 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -4.6 1.27)
		(size 2.3 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -4.6 3.81)
		(size 2.3 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 4.6 3.81)
		(size 2.3 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 4.6 1.27)
		(size 2.3 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 4.6 -1.27)
		(size 2.3 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 4.6 -3.81)
		(size 2.3 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Pressure.3dshapes/CFSensor_XGZP6897x.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
