(footprint "CFSensor_XGZP6899x"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Port External Dia 3mm, Port Internal Dia 1mm, 8 Pin (https://cfsensor.com/wp-content/uploads/2022/11/XGZP6899D-Pressure-Sensor-V2.8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py, hand modified")
	(tags "sop sensor")
	(property "Reference" "REF**"
		(at 0 7.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "CFSensor_XGZP6899x"
		(at 0 9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Port 1 (HP)"
		(at 2 -12.5 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "Port 2 (LP)"
		(at -2 -12.5 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -8.2 -3.81)
		(size 2.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.185185)
	)
	(pad "2" smd roundrect
		(at -8.2 -1.27)
		(size 2.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.185185)
	)
	(pad "3" smd roundrect
		(at -8.2 1.27)
		(size 2.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.185185)
	)
	(pad "4" smd roundrect
		(at -8.2 3.81)
		(size 2.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.185185)
	)
	(pad "5" smd roundrect
		(at 8.2 3.81)
		(size 2.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.185185)
	)
	(pad "6" smd roundrect
		(at 8.2 1.27)
		(size 2.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.185185)
	)
	(pad "7" smd roundrect
		(at 8.2 -1.27)
		(size 2.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.185185)
	)
	(pad "8" smd roundrect
		(at 8.2 -3.81)
		(size 2.4 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.185185)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Sensor_Pressure.3dshapes/CFSensor_XGZP6899x.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
