(footprint "Wells_648-0482211SA01"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "https://www.farnell.com/cad/316865.pdf?_ga=2.37208032.177107060.1530611323-249019997.1498114824")
	(tags "48pin TSOP Socket")
	(property "Reference" "REF**"
		(at 15.47 16 0)
		(layer "F.SilkS")
	)
	(property "Value" "Wells_648-0482211SA01"
		(at 15.47 -4.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 15.47 16 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -3.53 -1.75)
		(size 2 2)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 34.47 13.25)
		(size 2 2)
		(drill 1.7)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole roundrect
		(at -3.3 0.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "3" thru_hole roundrect
		(at 3.3 1)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "4" thru_hole roundrect
		(at 0 1.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "5" thru_hole roundrect
		(at -3.3 2)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "6" thru_hole roundrect
		(at 3.3 2.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "7" thru_hole roundrect
		(at 0 3)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "8" thru_hole roundrect
		(at -3.3 3.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "9" thru_hole roundrect
		(at 3.3 4)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "10" thru_hole roundrect
		(at 0 4.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "11" thru_hole roundrect
		(at -3.3 5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "12" thru_hole roundrect
		(at 3.3 5.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "13" thru_hole roundrect
		(at 0 6)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "14" thru_hole roundrect
		(at -3.3 6.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "15" thru_hole roundrect
		(at 3.3 7)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "16" thru_hole roundrect
		(at 0 7.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "17" thru_hole roundrect
		(at -3.3 8)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "18" thru_hole roundrect
		(at 3.3 8.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "19" thru_hole roundrect
		(at 0 9)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "20" thru_hole roundrect
		(at -3.3 9.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "21" thru_hole roundrect
		(at 3.3 10)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "22" thru_hole roundrect
		(at 0 10.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "23" thru_hole roundrect
		(at -3.3 11)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "24" thru_hole roundrect
		(at 3.3 11.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "25" thru_hole roundrect
		(at 27.64 11.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "26" thru_hole roundrect
		(at 34.24 11)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "27" thru_hole roundrect
		(at 30.94 10.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "28" thru_hole roundrect
		(at 27.64 10)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "29" thru_hole roundrect
		(at 34.24 9.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "30" thru_hole roundrect
		(at 30.94 9)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "31" thru_hole roundrect
		(at 27.64 8.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "32" thru_hole roundrect
		(at 34.24 8)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "33" thru_hole roundrect
		(at 30.94 7.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "34" thru_hole roundrect
		(at 27.64 7)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "35" thru_hole roundrect
		(at 34.24 6.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "36" thru_hole roundrect
		(at 30.94 6)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "37" thru_hole roundrect
		(at 27.64 5.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "38" thru_hole roundrect
		(at 34.24 5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "39" thru_hole roundrect
		(at 30.94 4.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "40" thru_hole roundrect
		(at 27.64 4)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "41" thru_hole roundrect
		(at 34.24 3.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "42" thru_hole roundrect
		(at 30.94 3)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "43" thru_hole roundrect
		(at 27.64 2.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "44" thru_hole roundrect
		(at 34.24 2)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "45" thru_hole roundrect
		(at 30.94 1.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "46" thru_hole roundrect
		(at 27.64 1)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "47" thru_hole roundrect
		(at 34.24 0.5)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "48" thru_hole roundrect
		(at 30.94 0)
		(size 1.5 1.1)
		(drill 0.75)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Socket.3dshapes/Wells_648-0482211SA01.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
