(footprint "TerminalBlock_Dinkle_DT-55-B01X-28_P10.00mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Dinkle DT-55-B01X Terminal Block  pitch 10.00mm https://www.dinkle.com/en/terminal/DT-55-B01W-XX")
	(tags "Dinkle DT-55-B01X Terminal Block  pitch 10.00mm")
	(property "Reference" "REF**"
		(at 135.08 -10.16 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_Dinkle_DT-55-B01X-28_P10.00mm"
		(at 135.08 10.16 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 135.08 -10.16 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 10 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 20 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 30 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 40 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 50 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 60 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 70 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at 80 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at 90 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at 100 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole oval
		(at 110 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole oval
		(at 120 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "14" thru_hole oval
		(at 130 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole oval
		(at 140 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "16" thru_hole oval
		(at 150 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole oval
		(at 160 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "18" thru_hole oval
		(at 170 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "19" thru_hole oval
		(at 180 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "20" thru_hole oval
		(at 190 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "21" thru_hole oval
		(at 200 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "22" thru_hole oval
		(at 210 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "23" thru_hole oval
		(at 220 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "24" thru_hole oval
		(at 230 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "25" thru_hole oval
		(at 240 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "26" thru_hole oval
		(at 250 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "27" thru_hole oval
		(at 260 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "28" thru_hole oval
		(at 270 0)
		(size 3.3 6.6)
		(drill 2.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Dinkle.3dshapes/TerminalBlock_Dinkle_DT-55-B01X-28_P10.00mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
