(footprint "TerminalBlock_WAGO_236-612_1x12_P10.00mm_45Degree"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Terminal Block WAGO 236-612, 45Degree (cable under 45degree), 12 pins, pitch 10mm, size 122x14mm, drill diameter 1.15mm, pad diameter 3mm, , script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_WAGO")
	(tags "THT Terminal Block WAGO 236-612 45Degree pitch 10mm size 122x14mm drill 1.15mm pad 3mm")
	(property "Reference" "REF**"
		(at 57.65 -6.12 0)
		(layer "F.SilkS")
	)
	(property "Value" "TerminalBlock_WAGO_236-612_1x12_P10.00mm_45Degree"
		(at 57.65 10.12 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(fp_text user "${REFERENCE}"
		(at 57.65 1 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.166667)
	)
	(pad "1" thru_hole rect
		(at 0 5)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 10 0)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 10 5)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 20 0)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 20 5)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 30 0)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 30 5)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 40 0)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 40 5)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 50 0)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 50 5)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 60 0)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole oval
		(at 60 5)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 70 0)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole oval
		(at 70 5)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at 80 0)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole oval
		(at 80 5)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at 90 0)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "10" thru_hole oval
		(at 90 5)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at 100 0)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole oval
		(at 100 5)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole oval
		(at 110 0)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "12" thru_hole oval
		(at 110 5)
		(size 1.5 3)
		(drill 1.15)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_WAGO.3dshapes/TerminalBlock_WAGO_236-612_1x12_P10.00mm_45Degree.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
