(footprint "TestPoint_2Pads_Pitch2.54mm_Drill0.8mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Test point with 2 pins, pitch 2.54mm, drill diameter 0.8mm")
	(tags "CONN DEV")
	(property "Reference" "REF**"
		(at 1.3 -2 0)
		(layer "F.SilkS")
	)
	(property "Value" "TestPoint_2Pads_Pitch2.54mm_Drill0.8mm"
		(at 1.27 2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 1.3 -2 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.54 0)
		(size 1.4 1.4)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
