(footprint "TestPoint_2Pads_Pitch5.08mm_Drill1.3mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Test point with 2 pads, pitch 5.08mm, hole diameter 1.3mm, wire diameter 1.0mm")
	(tags "CONN DEV")
	(property "Reference" "REF**"
		(at 2.54 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "TestPoint_2Pads_Pitch5.08mm_Drill1.3mm"
		(at 2.54 3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 2.54 0 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole roundrect
		(at 0 0)
		(size 2.6 2.6)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(roundrect_rratio 0.25)
	)
	(pad "2" thru_hole circle
		(at 5.08 0)
		(size 2.6 2.6)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
