(footprint "TestPoint_THTPad_2.5x2.5mm_Drill1.2mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "THT rectangular pad as test Point, square 2.5mm side length, hole diameter 1.2mm")
	(tags "test point THT pad rectangle square")
	(property "Reference" "REF**"
		(at 0 -2.148 0)
		(layer "F.SilkS")
	)
	(property "Value" "TestPoint_THTPad_2.5x2.5mm_Drill1.2mm"
		(at 0 2.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr exclude_from_pos_files exclude_from_bom)
	(fp_text user "${REFERENCE}"
		(at 0 -2.15 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2.5 2.5)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
)
