(footprint "Transformer_Coilcraft_CST2010"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Current sense transformer, SMD, 14.55x19.91x10.50mm (https://www.coilcraft.com/pdfs/cst2010.pdf)")
	(tags "Transformer current sense SMD")
	(property "Reference" "REF**"
		(at 0 -9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Transformer_Coilcraft_CST2010"
		(at 0 9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -9.04 -5.08)
		(size 2.34 1.19)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -9.04 -2.54)
		(size 2.34 1.19)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -9.04 0)
		(size 2.34 1.19)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -9.04 2.54)
		(size 2.34 1.19)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -9.04 5.08)
		(size 2.34 1.19)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 9.04 5.08)
		(size 2.34 1.19)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 9.04 2.54)
		(size 2.34 1.19)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 9.04 0)
		(size 2.34 1.19)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 9.04 -2.54)
		(size 2.34 1.19)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 9.04 -5.08)
		(size 2.34 1.19)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0 -5.62)
		(size 7.24 4.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 0 5.62)
		(size 7.24 4.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Transformer_SMD.3dshapes/Transformer_Coilcraft_CST2010.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
